MANUAL & ASSEMBLY INSTRUCTIONS

PLEASE READ ALL INSTRUCTIONS BEFORE OPERATING THIS APPERATUS.

* TO INCREASE LONGEVITY, PLEASE USE 25LB WEIGHT
* PLEASE USE IN A CONTROLLED SETTING
* DO NOT USE THIS APPERATUS FOR ANYTHING OTHER THAN ITS INTENDED PURPOSE

# YOUR ON-POINT ASSEMBLY KIT



# INSTRUCTION MANUAL

Use pictures for important points or important notions

|  |  |
| --- | --- |
| **NECESSARY ITEM:** | * **(1) ADJUSTABLE WRENCH NECESSARY FOR ASSEMBLY** |
|  | * **(2) ON-POINT VOLLEYBALL BOXES**  1. **34’’ x 32’’ x 4’’** 2. **67’’ x 7’’ x 2’’** |

|  |  |
| --- | --- |
|  | * **(1) VERTICAL INNER POLE (SILVER)** |
|  | * **(1) VERTICAL OUTER POLE (YELLOW)** |
|  | * **(1) BASE** |
|  | * **(5) NUTS** |
|  | * **(3) 3.5” BOLTS** * **(2) 3.2” BOLTS** |
|  | * **(16) VELCRO** |
|  | * **(1) 20” HOOP** |
|  | * **(1) 30” HOOP** |
|  | * **(1) TEMPO TARGET HEAD** |
|  | * **(2) NETS** |
|  | * **(1) ANGLE WHEEL** |

|  |  |
| --- | --- |
|  | * **(OPTIONAL) TOUCH-POINT ACCESSORY** |

# MANUAL & ASSEMBLY INSTRUCTIONS

## 

## Insert silver inner pre-drilled pole into yellow outer pole


## VERTICALLY PLACE ASSEMBLED POLE ON THE BASE






## line up outermost pre-drilled hole of the base with outermost pre-drilled hole of the yellow pole

1. SECURE POSITION BY SCREWING (3) 3.5” BOLTS AND (3) NUTS THROUGH BASE AND POLES





1. ATTACH ANGLE WHEEL BY LINING UP SILVER INNER POLE WITH OUTERMOST HEAD OF THE ANGLE WHEEL.
2. FASTEN WITH (2) 3.2” BOLTS AND (2) NUTS.



1. INSERT THE NECK OF THE ANGLE WHEEL INTO THE TARGET HEAD OF YOUR CHOICE AND
2. LINE THE PRE-DRILLED HOLES WITH THE LATCH PIN



1. SET DESIRED ANGLE WITH A LATCH PIN



1. ATTACH THE NET TO THE RIM OF THE HOOP BY USING 8 VELCRO STRAPS
2. CORRECT POSITIONING FOR THE METAL REINFORCEMENT PLATE ON 20” AND 30” TARGETS SHOULD ALWAYS BE FACE DOWN ON THE RIM.
3. FOR TOUCH-PONT ACCESSORY ONLY; SET TOUCH-POINT ON THE 7TH HOLE TO REACH 11FT TALL.



1. TO INCREASE LONGEVITY, PLEASE USE 25LB WEIGHT
2. PLEASE USE IN A CONTROLLED SETTING
3. DO NOT USE THIS APPERATUS FOR ANYTHING OTHER THAN ITS INTENDED PURPOSE

End of document